{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":75,"n_cols":13,"rows_kept":75,"merged":[[0,0,0,4],[1,0,1,4],[5,0,5,4],[13,0,13,4],[14,0,14,4],[18,0,18,4],[21,0,21,4],[24,0,24,4],[26,0,26,4],[31,0,31,4],[38,0,38,4],[51,0,51,4],[55,0,55,4],[59,0,59,4],[71,0,71,4]]}
["Солярий с ФР"]
["Подключение периферии к плате SK-MLPC2368",{"$nulls":4},"w64_01_Cross_v1"]
[]
[]
["№ порта",null,null,"№ на разъеме","Назначение"]
["ЖК индикатор MT-20S4M-2KLW-3V0 (в четырехбитном режиме, DB0-DB3 не подключаются)",{"$nulls":11},"вход"]
["P2.8",null,null,"MK_P65","Сигнал A0 индикатора",{"$nulls":7},"выход"]
["P2.7",null,null,"MK_P66","Сигнал E индикатора",{"$nulls":7},"опционная колодка"]
["P2.6",null,null,"MK_P67","Сигнал R_W индикатора"]
["P0.19",null,null,"MK_P59","DB4"]
["P0.20",null,null,"MK_P58","DB5"]
["P0.21",null,null,"MK_P57","DB6"]
["P0.22",null,null,"MK_P56","DB7"]
["Купюроприемник CashCode SM"]
["Модем подключается через приемопередатчик RS-232"]
["P2.1",null,null,"MK_P74","TXD-TTL"]
["P2.0",null,null,"MK_P75","RXD-TTL"]
["P2.4",null,null,"MK_P69","CCNET BUS RESET"]
["Монетоприемник NRI G-13"]
["P0.23",null,null,"MK_P9","IMPULSE OUTPUT (импульсный выход монетоприемника)"]
["P0.24",null,null,"MK_P8","INHIBIT (блокировка)"]
["Банковский терминал Vendotek",{"$nulls":6},"BH-40","BH-20","XP2"]
["P0.26","P0.26, RXD3",null,"MK_P6","IMPULSE OUTPUT (импульсный выход банк.терминала)",null,null,14]
["P0.25","P0.25, TXD3",null,"MK_P7","INHIBIT. Активный уровень LOW. При этом сигнале терминал блокируется",null,null,16]
["Фискальный регистратор Paykiosk"]
["Подключаем на разъем для COM-порта на плате."]
["Микросхема FRAM (память для хранения настроек и журнала)"]
["P0.18",null,null,"MK_P60","MOSI микросхемы FRAM"]
["P0.17",null,null,"MK_P61","MISO микросхемы FRAM"]
["P0.15",null,null,"MK_P62","SCK микросхемы FRAM"]
["P0.16",null,null,"MK_P63","CS микросхемы FRAM"]
["Клавиатура СК-15-1 (матричная 3х3)"]
["P2.3","GPIO P2.3",null,"MK_P70","\"1\"",{"$nulls":3},"КТ6"]
["P1.29","GPIO P1.29",null,"MK_P45","\"2\"",{"$nulls":3},"КТ12"]
["P2.13","GPIO P2.13",null,"MK_P50","\"3\"",{"$nulls":3},"КТ5"]
["P1.23","P1.23, MISO0",null,"MK_P37","\"a\"",{"$nulls":3},"КТ10"]
["P1.25","GPIO P1.25",null,"MK_P39","\"b\"",{"$nulls":3},"КТ1"]
["P1.24","P1.24, MOSI0",null,"MK_P38","\"c\"",{"$nulls":3},"КТ3"]
["Управление соляриями"]
["P3.26","GPIO P3.25",null,"MK_P27","Solarium 1. LAMP",null,null,12]
["P1.18","GPIO P1.19",null,"MK_P33","Solarium 1. VENT",null,null,8]
["P3.25","GPIO P3.26",null,"MK_P26","Solarium 1. Start",null,null,10]
["P1.19",null,null,"MK_P32","Solarium 1. Stop",null,null,6]
["P2.2","GPIO P2.2",null,"MK_P73","Solarium 2. LAMP",null,null,20]
["P0.4","GPIO P0.4",null,"MK_P81","Solarium 2. VENT",null,null,32]
["P0.5","GPIO P0.5",null,"MK_P80","Solarium 2. Start",null,null,26]
["P4.28","P4.28, TXD3",null,"MK_P82","Solarium 2. Stop",null,null,30]
["P1.27","GPIO P1.27",null,"MK_P43","Solarium 3. LAMP",null,null,36]
["P0.0","P0.0, TXD3",null,"MK_P46","Solarium 3. VENT",null,null,40]
["P1.28","GPIO P1.28",null,"MK_P44","Solarium 3. Start",null,null,34]
["P1.26","GPIO P1.26",null,"MK_P40","Solarium 3. Stop",null,null,38]
["Управление"]
["P1.20","P1.20, SCK0",null,"MK_P34","кнопка ОК",null,null,2]
["P1.21","P1.21, SSEL0",null,"MK_P35","управление подсветкой (кнопка ОК)",null,null,4]
["P1.22","GPIO P1.22",null,"MK_P36","выбор режима «работа»/«сервис»"]
[" RS-485"]
["P0.11","P0.11, RXD2, SCL2",null,"MK_P49","UART RXD2 - вход UART микроконтроллера",{"$nulls":4},"OP1","кинем провод"]
["P0.10","P0.10, TXD2, SDA2",null,"MK_P48","UART TXD2 - выход UART микроконтроллера",{"$nulls":4},"OP2","кинем провод"]
["P0.1","P0.1, RXD3, SCL1",null,"MK_P47","RTS - выход управления потоком для микросхемы RS-485",{"$nulls":3},"КТ4"]
["Звук (модуль WaveShare Music Shield)"]
["P0.6","P0.6, SSEL1",null,"MK_P79","SSEL1 - вход D10 модуля (CS SD-карты)",null,null,28]
["P0.7","P0.7, SCK1",null,"MK_P78","SCK1 - вход модуля D13 (SCLK)",null,null,22]
["P0.8","P0.8, MISO1",null,"MK_P77","MISO1 - выход D11 модуля (MISO)",null,null,24]
["P0.9","P0.8, MOSI1",null,"MK_P76","MOSI1 - вход D12 модуля (MOSI)",null,null,18]
["P2.11","GPIO P2.11",null,"MK_P52","вход A0 (XRESET) модуля",{"$nulls":3},"КТ14"]
["P1.31","P1.31, SCK1",null,"MK_P20","выход A1 (DREQ) модуля",{"$nulls":3},"КТ16"]
["P2.12","GPIO P2.12",null,"MK_P51","вход A2 (XDCS) модуля",{"$nulls":3},"КТ15"]
["P2.5","GPIO P2.5",null,"MK_P68","вход А3 (XCS) модуля",{"$nulls":3},"КТ7"]
[{"$nulls":4},"выход D9 (SD_Detect) модуля","не будем использовать"]
[]
[]
["Резерв"]
["P0.28","P0.28, SCL0",null,"MK_P24","Open drain output (for I2C-bus compliance)",{"$nulls":3},"KT11"]
["P0.27","P0.27, SDA0",null,"MK_P25","Open drain output (for I2C-bus compliance)",{"$nulls":3},"KT12"]
[null,"GPIO P2.10",null,"MK_P53","LOW on this pin while RESET is LOW forces on-chip bootloader to take over control of the part after a reset",{"$nulls":3},"КТ2"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}